{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Berechnung"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Berechnung","index":0,"n_rows":33,"n_cols":3,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,2],[6,1,6,2]],"flags":["formulas_cached_only"]}
["Tangentenberechnung einer Drehleier"]
[]
["Mensur",368,"mm"]
["Nach Pythagoras:",2]
["Eigene Versuche:",2.2055]
[]
[null,"Maße vom"]
[null,"Sattel aus","Steg aus"]
["g",368,0]
["gis",347.3503335218073,20.649666478192728]
["a",327.8593864068227,40.14061359317731]
["b",309.46213917572,58.53786082428002]
["h",292.0972208017888,75.90277919821119]
["c",275.70670398449545,92.29329601550455]
["cis",260.23591191090406,107.76408808909594]
["d",245.63323586033746,122.36676413966254]
["dis",231.84996304382872,136.15003695617128]
["e",218.84011410405597,149.15988589594403]
["f",206.5602897336799,161.4397102663201]
["fis",194.96952590042082,173.03047409957918]
["g",184.0291571959234,183.9708428040766]
["gis",173.70268785255732,194.29731214744268]
["a",163.95566999788088,204.04433000211912]
["b",154.75558874063938,213.24441125936062]
["h",146.07175370495852,221.92824629504148]
["c",137.8751966509039,230.1248033490961]
["cis",130.13857483988107,237.86142516011893]
["d",122.83607982251459,245.1639201774854]
["dis",115.94335134473312,252.05664865526688]
["e",109.43739608486177,258.5626039151382]
["f",103.29651095063822,264.7034890493618]
["fis",97.50021068028045,270.4997893197195]
["g",92.02915950609209,275.97084049390793]